SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( odos_771170
	comment( upravil Ondra Janis na zaklade poznatku o ladeni eng 
  souboru od Ppoolllla, Jacka, O.Frinty & ZSR  - verze 1.0 )
	comment( upravy brzd pro zvuky, svetla pro MSTSbin dle Jacka )
	Type ( Engine )
	WagonShape ( "odos_771170.s" )
	Size ( 3m 4.4m 16.94m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 115.8t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3m 4.4m 16.94m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

	Adheasion ( 0.18 0.73 1.94 0 )
  comment (melo by odpovidat adhezni sile pro 771 ~270kN (soucinitel adheze 0.23))
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*116t )
	DerailBufferForce ( 700kN )
comment( pocet naprav )
	NumWheels (	6 )
comment( sily urcujici jizdni odpory )
	Friction (
		4980N/m/s		0		0.625mph		1.07N/m/s		2.75
		5.1N/rad/s		1		-1rad/s		0		1
	)

  BrakeEquipmentType( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 69kN )
	comment(odpovida 61 brzdnym % v rezimu P - ZD 560m)

	MaxHandbrakeForce( 10kN )
	NumberOfHandbrakeLeverSteps( 100 )

	EmergencyBrakeResMaxPressure( 73 )
	TripleValveRatio( 2.48 )
	MaxReleaseRate( 1.5 )
	comment (brzda v rezimu P - odbrzdeni cca. 16s)
	MaxApplicationRate( 2 )
  comment (brzda v rezimu P - plneni cca. 5s)
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 0.02 )

	IntakePoint ( 0 1.0 FuelDiesel )

	PassengerCapacity ( 80.0 )
	Comment (kapacita cestujicich - jen kvuli tvorbe JR v misich)

	Lights ( 25
		Light (
			comment ( Svetelny kuzel dalkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
			  	Position ( 0.0 4.055 7.515 )
					Angle ( 20 )
					Transition ( 1 )
					Radius ( 100 )
				)
			)
		)
		Light (
			comment ( Svetelny kuzel tlumeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.0 2.0 7.5 )
					Angle ( 25 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)
		
		comment ( Definice svetel pro predni stanoviste )

		Light (
			comment ( reflektor dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.0 4.055 7.515 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.2 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60ff0000 )
					Position ( -0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60ff0000 )
					Position ( 0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment ( Definice svetel pro zadni stanoviste )

		Light (
			comment ( reflektor dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.0 4.055 -7.515 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.2 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60ff0000 )
					Position ( -0.58 2.065 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60ff0000 )
					Position ( 0.58 2.065 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Leve predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Prave predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 -7.31 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Prave zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 -7.31 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
			)
		)

		comment ( Definice svetel pro loko ovladanou PC )

		Light (
			comment ( PC predni prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.58 2.065 7.31 )
					Azimuth ( 0 -5 5 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC predni leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.58 2.065 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC reflektor predni )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
			  	Position ( 0.0 4.055 7.515 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.2 )
				)
			)
		)
		Light (
			comment ( PC zadni leve koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60ff0000 )
					Position ( -0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60ff0000 )
					Position ( 0.58 2.065 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
	)
    	Sound ("../../common.snd/snd771/771gceng.sms"  )
)

Engine ( odos_771170
	Effects (
		DieselSpecialEffects (
			Exhaust1
				(
					-0.201 4.55 -1.756
					0 1 0
					0.2
				)
		)
	)
	Wagon ( odos_771170 )
	Type ( Diesel )
	MaxPower ( 745kW ) 
      comment (vykon na obvodu kol - vypocteno z trakcni char.) 
	MaxForce ( 680kN )
	    comment (nejde o skutecne dosazitelnou (=adhezni) max. taznou silu, ale kompromis pro taznou silu na jednotlive stupne -
      pri tazne sile ~270kN (adheze 0.23) dojde k dosazeni meze adheze a prokluzu)
	RunUpTimeToMaxForce ( 40.0 )
	MaxContinuousForce ( 680kN )
	MaxVelocity ( 90km/h )
	MaxCurrent ( 8000A )
	comment (kompromis pro realnejsi ukazovani ampermetru; trvaly proud 2340A = 198kN tazne sily)
	WheelRadius ( 0.5m )
	Sanding ( 19km/h )
	NumWheels ( 6 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )
	DieselEngineSpeedOfMaxTractiveEffort( 15 km/h )
	
  AirBrakesAirCompressorPowerRating( 2.28 )
	AirBrakesMainMinResAirPressure( 68 )
	AirBrakesMainMaxAirPressure( 131 )
	AirBrakesMainResVolume( 35 )
	AirBrakesAirCompressorWattage( 30000 )
	AirBrakesCompressorRestartPressure( 113 )

	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.81 )
	EngineBrakesControllerMaxApplicationRate( 10 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerEmergencyApplicationRate( 15.0 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 73 )
	
  TrainBrakesControllerMinPressureReduction( 3 )	
	TrainBrakesControllerMaxApplicationRate( 2 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate ( 4 )
	TrainBrakesControllerEmergencyApplicationRate( 6 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	TrainBrakesControllerMaxSystemPressure( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 22.5 )
	TrainPipeLeakRate( 0.1 )
		
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
  BrakesEngineControllers( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent( 1 )

 	CabView ( "../../common.cab/cab771/771old.cvf" )
	HeadOut ( 1.7 3.25 -4.373 )

 	MaxDieselLevel ( 6000l )
	DieselUsedPerHourAtMaxPower ( 270l )
	DieselUsedPerHourAtIdle ( 28l )

	DieselSmokeEffectInitialMagnitude( 1.0 )
	DieselSmokeEffectMaxMagnitude( 2.0 )

	DieselSmokeEffectInitialSmokeRate( 0.7 )
	DieselSmokeEffectMaxSmokeRate( 2.2 )

	DieselEngineIdleRPM( 350 )
	DieselEngineMaxRPM( 750 )
  DieselEngineMaxRPMChangeRate( 25 )

	DoesHornTriggerBell( 0 )

	MaxSandingTime( 2000 )
	comment( 320kg )

	EmergencyStopMonitor(
    MonitoringDeviceMonitorTimeLimit( 0 )
    MonitoringDeviceAlarmTimeLimit( 0 )
    MonitoringDevicePenaltyTimeLimit( 0 )
    MonitoringDeviceCriticalLevel( 0 )
    MonitoringDeviceResetLevel( 0 )
    MonitoringDeviceAppliesFullBrake( 0 )
    MonitoringDeviceAppliesEmergencyBrake( 1 )
    MonitoringDeviceAppliesCutsPower( 1 )
    MonitoringDeviceAppliesShutsDownEngine( 1 )
    )

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 60 )
		MonitoringDeviceAlarmTimeLimit( 30 )
		MonitoringDevicePenaltyTimeLimit ( 20 ) 
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceTriggerOnOverspeed ( 64 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)
		
	OverSpeedMonitor(
		MonitoringDeviceTriggerOnOverspeed ( 73 )
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		)
		
	EngineVariables( 4000 )
			
        EngineControllers (
          Throttle ( 0 1 0.04 0
                NumNotches ( 9
                    Notch ( 0    0 Dummy )
		            		Notch ( 0.03 0 Dummy )
		            		Notch ( 0.07 0 Dummy )
		            		Notch ( 0.14 0 Dummy )
		            		Notch ( 0.30 0 Dummy )
			             	Notch ( 0.47 0 Dummy )
			             	Notch ( 0.65 0 Dummy )
			             	Notch ( 0.82 0 Dummy )
			             	Notch ( 1    0 Dummy )
                 )
            )
            Brake_Engine ( 0 0.76 0.125 0
                NumNotches( 1
                    Notch(0    1 Dummy )
                )
            )            
            comment(***Prubezna brzda typ DAKO-BS2***)            
           	Brake_Train ( 0 1 0.020 0.87
                NumNotches ( 7
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
                    Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
                    Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 1.00 0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
            NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )
            DirControl ( -1 0 1 1 )
            AWS ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
	        	Vigilance ( 0 1 0 )
	        	BailOffButton( 0 1 0 )
        )
        
      Name ("ODOS 771.170-8")
     	Description (
		"Rada 771 je dieselelektricka kapotova lokomotiva pro pouziti na tezky posun a vozbu nakladnich vlaku.\n\n"+
		"Usporadani dvojkoli: Co'Co'\n\n"+
		"Prenos vykonu: elektricky\n\n"+
		"Zdroj vykonu: naftovy motor CKD K 6 S 310 DR\n\n"+
    	"Jmenovity vykon motoru: 993 kW\n\n"+
    	"Trvala tazna sila: 198 kW\n\n"+
    	"Delka pres narazniky: 17,240 m\n\n"+
    	"Hmotnost: 115,8 t\n\n"+
    	"Max. rychlost: 90 km/h"
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestaveni reverzniho kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdeni vlakove brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.)\n"+
		"4.	Stisknete D pro zvyseni pozadovaneho vykonu.\n"+
		"5.	Pomalu zvysujte vykon stiskem D, dokud vlak nedosahne pozadovane rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jednim stiskem ' presunte vlakovou brzdu do polohy ZaVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snizeni pozadovaneho vykonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutne tak pouzijte brzdy pro postupne rychlejsi snizovani rychlosti.\n\n"+
		"Jak pouzit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosahnete pozadovaneho brzdneho tlaku.\n"+
		"2.	Po dosazeni pozadovaneho brzdneho tlaku stiskem ; presunte rukojet brzdy do polhy ZaVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENi.\n"+
		"2.	Pockejte, az klesne tlak v brzdovych valcich na 0.\n"+
		"3.	Po odbrzdeni a uvedeni vlaku do pohybu stisknete ' pro presunuti rukojeti brzdy do polohy ZaVER.\n\n"+
 		"Jak pouzit lokomotvni brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdeni lokomotivni brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivni brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy (0%).\n\n"+
		"Jak pouzit zachrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snizeni vykonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci zachrane brzdy.\n\n"+
		"Jak zrusit zachrannou brzdu\n"+
		"1.	Pockejte na uplne zastaveni vlaku.\n"+
		"2.	Stisknete Z pro odblokovani ovladani lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdeni brzdnych systemu.\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitym stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (pripadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Vystup a nastup cestujicich\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahajeni vystupu a nastupu cestujicich.\n"+
		"3.	Pockejte na signal k odjezdu.\n"+
		"TIP: Pro zobrazeni casu prijezdu a odjezdu u teto a nasledujici stanice pouzijte klavesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimalni rychlost 1 km/h).\n"+
		"Tip: Pro zobrazeni pohledu na sprahlo stisknete klavesu 6.\n"+
		"2.	Stisknete F9 pro otevreni okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervena, je zatazena rucni brzda. Dvojtukem mysi na voze uvolnite/zatahne rucni brzdu.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdite pripojene vozy.\n\n"+
		"Odpojeni vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJi!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se ma odpojit, pokud chcete, aby mel vuz zatazenou rucni brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftoveho stojanu stredem nadrze.\n"+
		"2.	Stisknete klavesu T a drzte ji po dobu doplnovani nafty stisknutou.\n"+
		"TIP: Pro zobrazeni prubehu plneni nadrze stisknete F9 a klepnete mysi na ikonu lokomotivy.\n\n"+
	)
	Sound ("../../common.snd/snd771/771gccab.sms"  )
)
