SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 31_54_7986_585_1_l_3082
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Max. rychlost 100" )
Comment ( "Josef Vogeltanz - 23.08.2018" )
Comment ( "Uprava - 03.01.2021" )

Comment ( "Obecne informace vozu" )
Type ( Freight )
WagonShape ( 31_54_7986_585_1.s )
Name ( "CDC Zaes 7986 585-1 dehet" )
Size ( 3.09m 4.29m 12.67m )
Mass ( 75.4t )
WheelRadius ( 0.46m )
ORTSNumberAxles ( 4 )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 0 )
WagonEmptyWeight ( 75.4t )
EmptyMaxBrakeForce ( 93kN )
EmptyMaxHandbrakeForce ( 16kN )

FreightAnimStatic (
SubType ( Default )
Shape ( bv_lo_3082.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 6.7e6N/m 4.4e8N/m ) Break ( 850kN 850kN ) r0 ( 0cm 0.1cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 850kN 850kN ) r0 ( 0cm 0.1cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 27/50t" )
Comment ( "Rezim brzdeni P")
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 93kN )
MaxHandbrakeForce ( 16kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.2bar/s )
MaxApplicationRate ( 0.45bar/s )
MaxAuxilaryChargingRate ( 1.216bar/s )
EmergencyResChargingRate ( 1.216bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 2.5 )
EmergencyResCapacity ( 100l )
BrakePipeVolume ( 12.1l )

ORTSBrakeShoeFriction (
0   0.310
8   0.238
16  0.193
24  0.168
32  0.152
40  0.140
48  0.131
56  0.123
64  0.116
72  0.109
80  0.105
88  0.101
96  0.098
104 0.096
112 0.094
120 0.093
128 0.092
136 0.092
144 0.092
152 0.092
160 0.092
)

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.12m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 1m 800mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 516.6 )
ORTSDavis_B ( 4.34 )
ORTSDavis_C ( 1.0182 )

Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//Vozy//CDvuzNakl4n-OR.sms" )
)